If you received ACK on floppy disk:

 Just type A:INSTALL or B:INSTALL to install ACK.

If you received ACK by modem:

 ACK normally includes two disks.  ACK installs best from floppy disk.
 If you must install from the hard drive, copy all the files into
 a directory called ACKINST.  But if you can, uncompress the files to
 two floppy disks and install ACK that way.

Vendors:

 You may distribute ACK freely so long as you encourage users to
 register, that you do not take or imply credit for my work, and that
 you use my installation utility -- don't make some goofy batch file --
 and that you tell people to "type A:INSTALL" on the label so the
 poor people at the software stores don't have to answer silly questions.

